Per Jesse’ direction calculation adjustments have been made.

Typar is 1 roll per 90 yards and fractions are increased to an additional roll if they are over .21 (add .79 to the calculations)

Yardage is adjusted to remove 50% on Materials and 90% on Labor.

I have tested both Pulte (Typar) lots and regular lots and the calculations seem to be correct.

This is of course provided they update from plans before they calculate.
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